TENDER TEXT
[bookmark: _GoBack]Furnish and install SMARTEMP® Perforated Multistream Wall Adjustable Diffusers, type PMW-AD, or equivalent, consisting of:
Front face made of perforated metal, located in an aluminium mounting frame, both painted to the colour specified.
Adjustable nozzles (manually rotatable via an Allen key inserted through the front face) made of plastic, located upstream of the front face, that produce a multitude of high and low momentum air streams of differing discharge direction. 
A galvanised perforated inlet plate located upstream of the nozzles.

